#!/bin/sh /etc/rc.common
# Copyright © 2012 OpenWrt.org
#
# This is free software, licensed under the GNU General Public License v2.
# See /LICENSE for more information.
#
START=70
STOP=30

USERS_C=/var/etc/nut/upsd.users
UPSD_C=/var/etc/nut/upsd.conf
UPS_C=/var/etc/nut/ups.conf

USE_PROCD=1

get_write_driver_config() {
	local cfg="$1"
	local var="$2"
	local def="$3"
	local flag="$4"
	local val

	[ -z "$flag" ] && {
		config_get val "$cfg" "$var" "$def"
		[ -n "$val" ] && [ "$val" != "0" ] && echo "$var = $val" >>"$UPS_C"
	}

	[ -n "$flag" ] && {
		config_get_bool val "$cfg" "$var" "$def"
		[ "$val" = 1 ] && echo "$var" >>"$UPS_C"
	}
}

upsd_statepath() {
	local statepath

	config_get statepath upsd statepath /var/run/nut
	STATEPATH="$statepath"
}

upsd_runas() {
	local runas

	[ -n "$RUNAS" ] && return 0

	config_get runas upsd runas nut
	RUNAS="$runas"
}

listen_address() {
    local cfg="$1"

    config_get address "$cfg" address "::1"
    config_get port "$cfg" port
    echo "LISTEN $address $port" >>"$UPSD_C"
}

upsd_config() {
    local cfg="$1"
    local maxage maxconn certfile runas statepath

    # Note runas support requires you make sure USB device file is readable by
    # the runas user
    config_get runas "$cfg" runas nut
    RUNAS="$runas"

    config_get statepath "$cfg" statepath /var/run/nut
    STATEPATH="$statepath"

    config_get maxage "$cfg" maxage
    [ -n "$maxage" ] && echo "MAXAGE $maxage" >>"$UPSD_C"

    [ -n "$statepath" ] && echo "STATEPATH $statepath" >>"$UPSD_C"

    config_get maxconn "$cfg" maxconn
    [ -n "$maxconn" ] && echo "MAXCONN $maxconn" >>"$UPSD_C"

    #NOTE: certs only apply to SSL-enabled version
    config_get certfile "$cfg" certfile
    [ -n "$certfile" ] && echo "CERTFILE $certfile" >>"$UPSD_C"
}

nut_user_add() {
	local cfg="$1"
	local a
	local val

	config_get val "$cfg" username "$1"
	echo "[$val]" >> "$USERS_C"

	config_get val "$cfg" password
	echo "  password = $val" >> "$USERS_C"

	config_get val "$cfg" actions
	for a in $val; do
	    echo "  actions = $a" >> "$USERS_C"
	done

	instcmd() {
		local val="$1"
		echo "  instcmds = $val" >> "$USERS_C"
	}

	config_list_foreach "$cfg" instcmd instcmd

	config_get val "$cfg" upsmon
	if [ -n "$val" ]; then
	    echo "  upsmon $val" >> "$USERS_C"
	fi
}

build_server_config() {
        mkdir -p "$(dirname "$UPSD_C")"
	chmod 0640 "$UPS_C"
	rm -f "$USERS_C"
	rm -f "$UPSD_C"
	rm -f /var/etc/nut/nut.conf

	echo "# Config file automatically generated from UCI config" > "$USERS_C"
	echo "# Config file automatically generated from UCI config" > "$UPSD_C"

	config_foreach nut_user_add user
	config_foreach listen_address listen_address
	config_foreach upsd_config upsd
	echo "MODE=netserver" >>/var/etc/nut/nut.conf

	chmod 0640 "$USERS_C"
	chmod 0640 "$UPSD_C"
	chmod 0644 /var/etc/nut/nut.conf

	[ -d "${STATEPATH}" ] || {
		mkdir -p "${STATEPATH}"
		chmod 0750 "${STATEPATH}"
	}

	if [ -n "$RUNAS" ]; then
		chown "$RUNAS":"$(id -gn "$RUNAS")" "${STATEPATH}"
		chgrp "$(id -gn "$RUNAS")" "$USERS_C"
		chgrp "$(id -gn "$RUNAS")" "$UPSD_C"
	fi
	haveserver=1
}

build_driver_config() {
	local cfg="$1"

	echo "[$cfg]" >>"$UPS_C"

	get_write_driver_config "$cfg" bus
	get_write_driver_config "$cfg" community
	get_write_driver_config "$cfg" desc
	get_write_driver_config "$cfg" driver "usbhid-ups"
	get_write_driver_config "$cfg" ignorelb 0 1
	get_write_driver_config "$cfg" interruptonly 0 1
	get_write_driver_config "$cfg" interruptsize
	get_write_driver_config "$cfg" maxreport
	get_write_driver_config "$cfg" maxstartdelay
	get_write_driver_config "$cfg" mfr
	get_write_driver_config "$cfg" model
	get_write_driver_config "$cfg" nolock 0 1
	get_write_driver_config "$cfg" notransferoids 0 1
	get_write_driver_config "$cfg" offdelay
	get_write_driver_config "$cfg" ondelay
	get_write_driver_config "$cfg" pollfreq
	get_write_driver_config "$cfg" port "auto"
	get_write_driver_config "$cfg" product
	get_write_driver_config "$cfg" productid
	get_write_driver_config "$cfg" retrydelay
	get_write_driver_config "$cfg" sdorder
	get_write_driver_config "$cfg" sdtime
	get_write_driver_config "$cfg" serial
	get_write_driver_config "$cfg" snmp_version
	get_write_driver_config "$cfg" snmp_retries
	get_write_driver_config "$cfg" snmp_timeout
	get_write_driver_config "$cfg" synchronous
	get_write_driver_config "$cfg" vendor
	get_write_driver_config "$cfg" vendorid

	# Params specific to NetXML driver
        get_write_driver_config "$cfg" login
        get_write_driver_config "$cfg" password
        get_write_driver_config "$cfg" subscribe 0 1

	defoverride() {
		local overvar="$1"
		local defover="$2"
		local overtype="$(echo "$overvar" | tr '_' '.')"
		local overval

		config_get overval "${defover}_${overvar}" value
		[ -n "$overval" ] && echo "${defover}.${overtype} = $overval" >>"$UPS_C"
	}

	config_list_foreach "$cfg" override defoverride override
	config_list_foreach "$cfg" default defoverride default

	other() {
		local othervar="$1"
		local othervarflag="$2"
		local otherval

		if [ "$othervarflag" = "otherflag" ]; then
			config_get_bool otherval "${othervarflag}_${othervar}" value
			[ "$otherval" = "1" ] && echo "${othervar}" >>"$UPS_C"
		else
			config_get otherval "${othervarflag}_${othervar}" value
			[ -n "$otherval" ] && echo "${othervar} = $otherval" >>"$UPS_C"
		fi
	}

	config_list_foreach "$cfg" other other other
	config_list_foreach "$cfg" otherflag other otherflag
	echo "" >>$UPS_C
	havedriver=1
}

build_global_driver_config() {
	local cfg="$1"

	# Global driver config
	get_write_driver_config "$cfg" chroot
	get_write_driver_config "$cfg" driverpath
	get_write_driver_config "$cfg" maxstartdelay
	get_write_driver_config "$cfg" maxretry
	get_write_driver_config "$cfg" retrydelay
	get_write_driver_config "$cfg" pollinterval
	get_write_driver_config "$cfg" synchronous
	config_get runas "$cfg" user nut
	RUNAS="$runas"

	echo "" >>"$UPS_C"
}

build_config() {
	local STATEPATH=/var/run/nut

        mkdir -p "$(dirname "$UPS_C")"
	rm -f "$UPS_C"
	echo "# Config file automatically generated from UCI config" > "$UPS_C"
	chmod 0640 "$UPS_C"

	config_load nut_server

	upsd_runas
	config_foreach build_global_driver_config driver_global
	config_foreach build_driver_config driver
	upsd_statepath
	build_server_config
	[ -n "$RUNAS" ] && chgrp "$(id -gn "$RUNAS")" "$UPS_C"
}

start_driver_instance() {
	local cfg="$1"
	local requested="$2"
	local driver
	local STATEPATH=/var/run/nut
	local RUNAS=nut

	[ "$havedriver" != 1 ] && return

	# If wanting a specific instance, only start it
	if [ "$requested" != "$cfg" ] && [ "$request" != "" ]; then
		return 0
	fi

	mkdir -p "$(dirname "$UPS_C")"
	chmod 0755 "$UPS_C"

	upsd_statepath
	build_config

	# Avoid hotplug inadvertenly restarting driver during
	# forced shutdown
	[ -f /var/run/killpower ] && return 0
	if [ -d /var/run/nut ] && [ -f /var/run/nut/disable-hotplug ]; then
	       return 0
	fi

	if [ -n "$RUNAS" ]; then
		chown "$RUNAS":"$(id -gn "$RUNAS")" "${STATEPATH}"
		chgrp "$(id -gn "$RUNAS")" "$UPS_C"
	fi

	config_get driver "$cfg" driver "usbhid-ups"
	procd_open_instance "$cfg"
	procd_set_param respawn
	procd_set_param stderr 0
	procd_set_param stdout 1
	procd_set_param command /lib/nut/"${driver}" -D -a "$cfg" ${RUNAS:+-u "$RUNAS"}
	procd_close_instance
}

interface_triggers() {
	local action="$1"
	local triggerlist trigger

	config_get triggerlist upsd triggerlist

	. /lib/functions/network.sh

	if [ -n "$triggerlist" ]; then
		for trigger in $triggerlist; do
			if [ "$action" = "add_trigger" ]; then
				procd_add_interface_trigger "interface.*" "$trigger" /etc/init.d/nut-server reload
			else
				network_is_up "$trigger" && return 0
			fi
		done
	else
		if [ "$action" = "add_trigger" ]; then
			procd_add_raw_trigger "interface.*.up" 2000 /etc/init.d/nut-server reload
		else
			ubus call network.device status | grep -q '"up": true' && return 0
		fi
	fi
	[ "$action" = "add_trigger" ] || return 1
}

start_server_instance() {
	local cfg="$1"

	[ "$haveserver" != 1 ] && return
	interface_triggers "check_interface_up" || return

	procd_open_instance "$cfg"
	procd_set_param respawn
	procd_set_param stderr 0
	procd_set_param stdout 1
	procd_set_param command /usr/sbin/upsd -D ${RUNAS:+-u "$RUNAS"}
	procd_close_instance
}

start_service() {
	local STATEPATH=/var/run/nut

	# Avoid hotplug inadvertenly restarting driver during
	# forced shutdown
	[ -f /var/run/killpower ] && return 0

	config_load nut_server
	build_config

	case $@ in
	"")
		config_foreach start_driver_instance driver "$@"
		start_server_instance upsd
		;;
	*upsd*)
		start_server_instance upsd
		;;
	*)
		config_foreach start_driver_instance driver "$@"
		;;
	esac
}

reload_service() {
	stop_service "$@"
	sleep 2
	start_service "$@"
}

service_triggers() {
	config_load nut_server

	interface_triggers "add_trigger"
	procd_add_reload_trigger "nut_server"
}
