From d41dc2046dd08d8c95197f677e224506f5b39bdd Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 20 Jan 2016 16:00:37 +0000
Subject: [PATCH 3/4] Increase firmware load timeout to 30s

---
 tools/hciattach.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/tools/hciattach.c
+++ b/tools/hciattach.c
@@ -1227,7 +1227,7 @@ int main(int argc, char *argv[])
 {
 	struct uart_t *u = NULL;
 	int detach, printpid, raw, opt, i, n, ld, err;
-	int to = 10;
+	int to = 30;
 	int init_speed = 0;
 	int send_break = 0;
 	pid_t pid;
